00.20.40.60.8105 0 1 0 0 1 5 0 2 0 0n-side after irradiationp-side after irradiation

Efficiency at Threshold 1fCBias Voltage [V]