8 68 89 09 29 49 69 81 0 0-20-1001 02 0

@1fC THRESHOLD, B=1.56T

ATT8- non-irradiatedATT7-irradiated

TRACKING EFFICIENCY [%]ROTATION ANGLE [o]